**Inconsistencies Breakdown:**

* **CONOPS vs. SRS:** The CONOPS explicitly states a need for **real-time notifications and alerts on a smartphone**, but the SRS (REQ-1.4) only specifies an **audible alarm**. This is a **major gap** between the user's needs and the specified requirements.
* **SRS vs. SDD:** The SRS (REQ-1.4) requires an alarm, and the SDD has an **Audio Alert Module** to fulfill this. However, the SDD's design decision to **not support external integrations** directly conflicts with the user need identified in the CONOPS, which means the SRS is incomplete. The SDD also introduces a **proprietary data format**, but the SRS provides no requirements for this.
* **SDD vs. V&V Plan:** The SDD describes a **Wi-Fi Communication Module** and its function, but the V&V Plan does not include a test case to **verify the encryption** required by NFR-2.2. A test for REQ-1.2 exists, but it only validates the connection, not the security attribute.